We have sent on 21 Dec 2012:
21.12.2012        WELDING Generator 400 W  LCD    3 pieces
21.12.2012        AMMM Generator 400 W  LCD    1 pieces
21.12.2012        AMMM Generator 400 W  LCD DRILLING for Posalux    1 pieces
21.12.2012        WELDING Generator 1000 W INOX BOX EUROSONIC    5 pieces
21.12.2012        CLEANING Generator 1000 W  INOX BOX EUROSONIC    2 pieces

We have sent on 27 Dec 2012:
27.12.2012        AMMM Generator 400 W  LCD DRILLING for Posalux    9 pieces
27.12.2012        AMMM Generator 400 W  LCD 115 V(American client from Boeing)    1 pieces
27.12.2012        WELDING Generator 1000 W  LCD    3 pieces
27.12.2012        AMMM Generator 1000 W  LCD    3 pieces

**-----------------------------------------------------------------**

.....explanations regarding low voltage cleaning generators:
 - we have sent two types of cleaning generators - one is low voltage and one is high voltage
 -for the low voltage generator - the output transformer voltage is low, because the generator is designed for low voltage transducer(immersible transducers and multi transducer baths)
 -the tubulartransducer you cannot drive with the low voltage, but with the high voltage cleaning generator, that can also drive single transducer loads.

 -how fast you can make 2 and 3 kW… for cleaning - minimum one month - I have already preliminary preparations as schematics and the main part of the PCBs, but as I told you I need good feedback for the present cleaning generators to avoid week points and malfunctions for the high power.

---------------------------------------------------------------------------------------------------------------

Inox welding generators are 100% the same as latest version generators, except voltages can be changed by software… is it something else different.  Please confirm? YES. Nothing else different. The latest software version is on the ftp.

When you send me AMMM 400W drilling generators, can I use and sell them also as the latest 400W, AMMM, or this is only and specifically for Posalux?  Please make comments.YES. You can use them as AMMM. BE CAREFULL, BECAUSE ONE OF THE 400W GENERATORS IS 115V FOR THE AMERICAN CLIENT.

 -------------------------------
When you will send me 3 kw generators?  How many? I am sending 3 pieces 3 kW generators as I told you(the others are too old and to repair like new means to produce new) and 1 pieces repaired EUROSONIC. I have also received from you one more 1 kW generator, but it is too broken and I will need time to repair, that's why I am not sending it now.

Good to hear from you, that you are getting better, use warm rakia for acceleration ....:)).  Also good to hear that the business is going well.

I also have some proposals and comments, but I will write later this week.I am trying to put our ideas and visions in order and later to discuss.

-----------------------------------

On our FTP server you have new software.  I need to update manuals and web site, regarding software.

Inside of AMMM software you have new files (not the same as presently on my web site).  What shall I use.  Is the latest AMMM software 100% compatible with what I have until today.  Please explain…  Do I need to upload new AMMM software files on the web site?  What ar5e the differences…
There is not difference between what you have on your website, I have just uploaded it when you asked me last time to put again last versions on the ftp.

Inside of ModBUS\_Soft  there is an empty folder … (you did not upload … or mistake…).  Please comment?

This is not a mistake, but when I created the directory ModBus there still was not ready software for upload. Now we have and I am uploading it today. The ModBus software is prepared to replace one day the other two types of software AMMM and WELDING, but when we all are ready to make it official- usermanuals, feedback from working generators, etc. Now it is for internal use only - you and me and Lalyo.

Welding\_Soft:  For welding part, looks to me that on the web site is the same software (nothing new).  Only “welding\_INOX\_1000W\_18122012” is new… give me some comments.
Exactly. The INOX software is only for the last Inox generators that are for Eric. The difference is that it is possible, when you choose type of generator "1kW inox", the function for "voltage select" is working(there are additional relays for the voltage inside the generator) - as Eric asked for.

I updated the welding generator manual for clients who will use it as SONICATOR… you can see few of new pages… This OK... Only the Usermanual becomes bigger and bigger, may be it is good to make simple short manuals for every type.